Wing Dihedral..................14 degrees each panel
Horizontal Tail Dihedral......8 degrees each panel
Incidence Settings.......... 0/0
Use 3/32 inch balsa for wing panels
Use 1/32 inch balsa for all tail surfaces